**Dave Dent, Livermore, CA: “**I have tried [Never Wet] on one of my blades on my Velocity and I was very disappointed with it. First of all it goes on very rough, and you have to put on two to three layers of the first step and wait to dry between layers. Then put on two layers of the second step. Making it very heavy. It works as far as not having anything stick to it. No oils, exhaust, etc. But I would not recommend it on the plans other then inside the cowl to prevent oils from sticking. I bought mine on Amazon but I went into Home Depot and saw it. The clerk at the store told me they will be sending it back because many people were disappointed with it - mainly because of the application method. It may be OK if not sprayed on with their spray can. I haven't put any in a cup and then into my spray gun. I have yet to try it.”